




Pc0 default gateway




Pc0 ip config




Pc default gateway




Pc1 ip config and subnet




Ip config r0




Serial 0/1/0 for r0




Ip config r1




Serial 0/1/0 for r1



Ripv2 commands for r0



Ripv2 commands for r1



Message successfully passed between pc0 to pc1